**BLINKING LED AND TRAFFIC LIGHT FOR RASPBERRY PI**

**NAME ; DEVA DHARSHINI**

**REG NO; 611819106006**

**ECE FINAL YEAR 7TH SEM**

**ASSIGMENT "3"**

------------------

import RPi.GPIO as GPIO

import time

#assign numbering for the GPIO using BCM

GPIO.setmode(GPIO.BCM)

#assingn number for the GPIO using Board

#GPIO.setmode(GPIO.BOARD)

cnt = 0

MAIL\_CHECK\_FREQ = 1 # change LED status every 1 seconds

RED\_LED = 4

GPIO.setup(RED\_LED, GPIO.OUT)

while True:

ifcnt == 0 :

GPIO.output(RED\_LED, False)

cnt = 1

else:

GPIO.output(RED\_LED, True)

cnt = 0

time.sleep(MAIL\_CHECK\_FREQ)

GPIO.cleanup()